;
; mosuSrPt.INF
; USB-to-Serial & USB-to-Parallel Windows98se Driver
;

[Version]
Signature="$CHICAGO$"
Class=Ports
ClassGUID={4d36e978-e325-11ce-bfc1-08002be10318}
Provider=%ProviderName%
;CatalogFile=mosuSrPt.cat
DriverVer=05/04/2006,1.8.5.11

[SourceDisksNames]
1=%DriversDisk%,,,

[SourceDisksFiles]
mosuSrPt.inf=1

[DestinationDirs]
DefaultDestDir=11

; Install class "Ports"
;----------------------------------------------------------
[ClassInstall]
AddReg=PortsClass.AddReg

[PortsClass.AddReg]
HKR,,,,%PortsClassName%

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%MfgName%=mosuSrPtHW

[mosuSrPtHW]
%MosSerPort.DeviceDesc%=mosuSrPt,MOSCHIP\COMPOUND_SERIAL_INTERFACE
%MosParPort.DeviceDesc%=mosuPrPt,MOSCHIP\COMPOUND_PARALLEL_INTERFACE

;---------------------------------------------------------------;
; For Win98 ...
;

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;; Serial Port Install Section
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;

[mosuSrPt]
AddReg=mosuSrPt.AddReg,mosuSrPt.W98.AddReg

[mosuSrPt.AddReg]
HKR,,PortSubClass,1,01

[mosuSrPt.W98.AddReg]
HKR,,DevLoader,,*vcomm
HKR,,PortDriver,,MOSUSRPT.vxd
HKR,,ConfigDialog,,serialui.dll
HKR,,Enumerator,,MCSENUM.vxd
HKR,,DCB,3,1C,00,00,00, 80,25,00,00, 11,33,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,,DisablePowerManagement,1,01,00,00,00
HKR,,PortSubClass,1,01
;;HKR,,EnumPropPages,,"serialui.dll,EnumPropPages"
HKR,,EnumPropPages,,MOSUSER.dll
HKR,,Icon,,102


;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;; Parallel Port Install Section
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;

[mosuPrPt]
AddReg=mosuPrPt.AddReg,mosuPrPt.W98.AddReg

[mosuPrPt.AddReg]
HKR,,PortSubClass,1,00

[mosuPrPt.W98.AddReg]
HKR,,DevLoader,,*vcomm
HKR,,PortDriver,,mosuPrPt.vxd
HKR,,PortSubClass,1,00
HKR,,ECPDevice,1,00
;;HKR,,EnumPropPages,,"serialui.dll,EnumPropPages"
HKR,,EnumPropPages,,MOSUPAR.dll
HKR,,Icon,,102


;---------------------------------------------------------------;

[Strings]
ProviderName="MosChip Semiconductor Technology"
MfgName="MosChip Semiconductor Technology"
PortsClassName = "Ports (COM & LPT)"
DriversDisk="USB-to-Serial Drivers Disk"
;USB\VID_9710&PID_7720.DeviceDesc="USB-to-Serial Port Driver"
MosSerPort.DeviceDesc="USB-to-Serial Port Driver"
MosParPort.DeviceDesc="USB-to-Parallel Port Driver"
USB\VID_9710&PID_7720.FriendlyName="USB-to-Serial FriendlyName"
